=====================================================================
	         Yafuflash Utility Instructions
=====================================================================
We provide several DOS mode batch files for you to update the BMC firmware version, 
as explained below:

1.
FLASH1.BAT : 
run this batch file to flash the BMC firmware and preserve most of the BMC settings.

2.
FLASH2.BAT : 
run this batch file to flash the BMC firmware and force BMC bootloader upgrade. 
Its do not preserve any BMC settings.

3.
FLASH3.BAT : 
run this batch file to flash the BMC firmware from BMC 1.0 series and BMC 2.0 series to BMC 2.2 series. 
Its do not preserve any BMC settings.
More notification please see "BMC 2.2 firmware series notification.txt"

4.
ASMB_MAC.exe and ASMC8.exe:
Subprogram for BMC firmware update.

5.
VSTR and XGREP:
Subfunction for FLASH3.BAT

6. 
*.ima : 
Image file of BMC firmware.



If you encounter any problems during the BMC firmware update process, please contact your system
vendor or ASUS Customer Service for support.
